## Using Your DDK

[prev][next][parent][TOC]

### DBCS 16-Bit Parallel Port Driver

Driver Description:

This 16-bit Parallel Port Printer Driver provides communication support for ISA and Micro Channel parallel ports.

Compilers/Assemblers Required:

         Microsoft MASM 5.1  (supplied with the DDK)

Build Instructions:

1.Run the SETDBCS.CMD command file in the <drive>:\DDK\TOOLS directory, passing <drive> and DDK as parameters. This will set the path and environment variables.

    e.g., SETDBCS <drive>:\DDK

Where <drive> represents your DDK installed drive and DDK represents the DDK installed directory. On the CD-ROM, the TOOLS directory path is DDK\ TOOLS.

2.Change the directory to DDK\DBCS\SRC\DEV\PRINTER.

3.Invoke NMAKE on the resident makefile.

Files Created by Successful Build:

         Directory:  \DDK\DBCS\SRC\DEV\PRINTER

         o  PRINT01.SYS
         o  PRINT02.SYS