## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SET_DRIVER

The SET_DRIVER command is used to configure a 32-bit display driver for use by the 32-bit graphics engine. The parameters associated with this keyword will be listed in the lines that follow the SET_DRIVER command. These parameters are passed to the DspSetDriverInfo function.

The format of the SET_DRIVER command line is :SET_DRIVER. Each parameter is specified as a <keyword> = <value> pair.

The following lists the parameters that must be specified in the lines following the SET_DRIVER command line. All the parameter values in this list are strings and must be enclosed in double quotation marks.

NAME = "<Name of display driver>"
DESC = "<String that describes display driver (can be NULL)>"
PATHNAME = "<Name of display driver>"
PARMS = "<String containing parameters for driver (can be NULL)>"

Following is an example of how to specify the parameter values used with the SET_DRIVER keyword command:

        :SET_DRIVER
        NAME="IBMVGA32"
        DESC="IBM VGA Display Driver"
        PATHNAME="IBMVGA32"
        PARMS=""