## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### Running the Sample Device Driver

The easiest way to install and run this sample device driver is to install Sigma Designs' ReelMagic through the OS/2 Warp Selective Install and copy this sample device driver over the Sigma Design Reel Magic device driver that has the same name. The file can be found in the MMOS2 subdirectory ( usually \MMOS2\VIDRMS1.SYS).

This device driver will not display images on the screen because it contains no hardware-specific code, but it will allow you to see and follow the commands and data to the device driver.

Reboot the computer after installing this sample device driver.