## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Request Packet Command Summary

The command code field of a request packet contains the function requested of the physical device driver. The parallel port device driver is a character device driver and supports all character device driver functions.

A detailed description of these commands can be found in the OS/2 Physical Device Driver Reference.