## Physical Device Driver Reference

[prev][next][parent][TOC]

### ASYNC_EXTGETBAUDRATE (63h) - Maximum Bit Rate Supported

Maximum Bit Rate Supported The binary integer representing the maximum bit rate (in bits-per-second) supported for a COM port. Depending on overall system overhead and the electrical characteristics of the hardware cables and serial device adapter type, the actual value of the maximum bit rate supported might be lower than this.