## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### ALP3522: Selected processor does not support this instruction

A mnemonic or mnemonic/operand combination has been used that is not supported by the processor for which the assembler is currently generating object code.

Recovery: Verify that the correct target processor has been selected with one of the processor selection directives, or that the correct instruction form has been coded. Since ALP does not perform some of the same implicit conversions that MASM 5.10 does, use of the <type> PTR conversion operator may be required to avoid certain type-mismatch problems.