## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Notes

FLDCW is typically used to establish or change the FPU's mode of operation.

If an exception bit in the status word is set, loading a new control word that unmasks that exception will result in a floating-point error condition . When changing modes, the recommended procedure is to clear any pending exceptions before loading the new control word.