## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PM Device Font Drivers

The PM device font driver is the 16-bit DLL that supplies SBCS and DBCS fonts to a PM display driver. The IBM Developer Connection Device Driver Kit for OS/2 includes source code for the following font drivers:

PMNLSFD1.FDR-MINCHO System Font Driver

PMNLSFD2.FDR-MINCHO Draft Font Driver

PS55DM28.FDR-MINCHO 28-dot Font Driver

PS55DM32.FDR-MINCHO 32-dot Font Driver

PS55DM36.FDR-MINCHO 36-dot Font Driver

PMNLSFD3.FDR-GOTHIC System Font Driver

PS55DG28.FDR-GOTHIC 28-dot Font Driver

PS55DG32 FDR-GOTHIC 32-dot Font Driver

PS55DG36.FDR-GOTHIC 36-dot Font Driver

Refer to Device Driver Font Manager Interface for details of the interface to the font drivers.