## Physical Device Driver Reference

[prev][next][parent][TOC]

### RMParseSCSIInquiry - Calling Parameters

InquiryData (PVOID) - output Pointer to a buffer containing SCSI inquiry data for the device.

DescBuffer (PSZ) - input Pointer to a buffer that will receive the device key and device description built by this service. This data may be used as the device description field (DevDescriptName) of the DEVICESTRUCT used to create the device.

Refer to RMCreateDevice for further information.

DescBufferSize (USHORT) - input Size of the DescBuffer, in bytes.

rc (APIRET) - returns On systems where the Resource Manager driver is not installed, the library interface code will return RMRC_NOT_INSTALLED.

RMRC_NULL_POINTER A Resource Manager service received a NULL value for a pointer that was expected to contain a valid 16:16 address.
RMRC_BUFFER_TOO_SMALL The buffer provided to receive information from a Resource Manager service was too small.