## Physical Device Driver Reference

[prev][next][parent][TOC]

### Status - TOUCH_DEVDEP_READDATA (53h)

Status Has the following bit-level definitions for XYZ mode:

Bit Description

0 1=Hardware offset adjust error

1 1=Offset adjust error

2 1=Floating point calculation error

3 Reserved=0

4 1=Channel pegged error

5 1=Offset adjust just occurred

6 Reserved=0

7 Reserved=0

8 Reserved=0

9 Reserved=0

A Reserved=0

B Reserved=0

C Touch screen status 2

D Touch screen status 1

E 1=Selection detection on

F 0=XYZ packet