## Physical Device Driver Reference

[prev][next][parent][TOC]

### SCREENDD_SETCURRENTBANK (01h) - Set Current Video Memory Bank

Category:
SCREENDD_CATEGORY (80h)
Function:
SCREENDD_SETCURRENTBANK (01h)
Description:
Set Current Video Memory Bank

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format
    Returns
    Remarks

This function sets the current video memory bank.