## Physical Device Driver Reference

[prev][next][parent][TOC]

### OEMHLP_GETVIDEOFONTS (03h) - Remarks

This function returns pointers to the video fonts through INT 10h (AH=1130h ).

Pointers returned by this IOCtl are addressed running in real mode. These pointers must then be converted to addresses running in protected mode before the applications and device drivers can access them.

Refer to the IBM Personal System/2 and Personal Computer BIOS Interface Technical Reference or the technical reference for your personal computer for more information about these pointers.