## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### SHD_REPORTINT

This data structure contains fields for the SHD_REPORT_INT message.

    typedef struct _shd_reportint_parm {

      ULONG       ulFunction;    /*  Function requested by PDD. */

      HSTREAM     hStream;       /*  Stream handle. */

      PVOID       pBuffer;       /*  Return pointer to last used buffer. */

      ULONG       ulFlag;        /*  Reason for interrupt. */

      ULONG       ulStatus;      /*  Return code or bytes read/written. */

      ULONG       ulStreamTime;  /*  Time in milliseconds of stream position. */

    } SHD_REPORTINT;

    typedef   SHD _ REPORTINT   * PSHD _ REPORTINT ;