## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Notes

The operand-size attribute has no effect on this instruction. This instruction is provided for compatibility with the Intel286 processor; programs for the Intel386, Intel486, and Pentium processors should use the MOV CR0, ... instruction instead. The LMSW instruction does not affect the PG, ET, or NE bits, and it cannot be used to clear the PE bit.