## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Hardcopy Device Names

If a hardcopy driver supports multiple devices, this is indicated at the API and user level. There are three parts:

The hardcopy driver implements OS2_PM_DRV_DEVICENAMES.

The hardcopy driver accepts a device name in the szDeviceName field of pdriv. See FillPhysicalDeviceBlock.

The device name is accepted in OS2_PM_DRV_DEVMODE.