## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### RGB2 Field - fcOptions

fcOptions (BYTE) Entry options.

These can be ORed together if required:

PC_RESERVED The color entry is reserved for animating color with the palette manager.

PC_EXPLICIT The low-order word of the color table entry designates a physical palette slot. This allows an application to show the actual contents of the device palette as realized for other logical palettes. This does not prevent the color in the slot from being changed for any reason.