## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SDBitBlt

Select an item:

    Syntax
    Parameters
    Returns
    Glossary

Simulation support:

This function is simulated by a handling routine in Revision 2.X of the graphics engine.

Description:

SDBitBlt is a preclipped BitBlt rendering routine. It processes BitBlt operations using all ROPs and common hardware mixes from Source/Pattern linear addresses to a Destination linear address. SDBitBlt is the default when OS2_PM_DRV_ENABLE: QueryDeviceSurface does not hook the pfnBitBlt function directly.

    #include <os2.h>

    PBITBLTINFO    pInput;   /*  Pointer to BITBLTINFO data structure. */

    PVOID          pOutput;  /*  Reserved. */

    ULONG          rc;       /*  Return codes. */

    rc = SDBitBlt(pInput, pOutput);