## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### The Target

The target runs on three kinds of operating systems:

The OS/2 target enables an OS/2 workstation to be monitored and controlled by the controller.

The Windows target enables a Windows workstation to be monitored and controlled by the controller. The controller connects to the workstation whether it is operating in DOS full-screen mode or in a Windows graphic environment.

The DOS target enables a DOS workstation to be monitored and controlled by the controller. To install the DOS target, either create an installation package or use the CID method. Use the packager on an OS/2 workstation to create a DOS target installation package and then install the target on the DOS workstation.

In each case, the controller connects to the target directly if it is a basic DCAF target, or through a gateway if the workstation is secure.