## Physical Device Driver Reference

[prev][next][parent][TOC]

### RMSetSnoopLevel

Select an item:

    Calling Sequence
    Calling Parameters
    Returns
    Remarks
    Glossary

This rminfo service sets the snoop level for the system. RMSaveDetectedData must save the previous.dat file before RMSetSnoopLevel can set the snoop level.

    #include <os2.h>

    #include <rmcalls.h>

    USHORT    SnoopLevel;

    USHORT    SnoopFlags;

    APIRET    rc;

    rc = RMSetSnoopLevel(SnoopLevel, SnoopFlags);