## Graphics Adapter Device Driver Reference

[prev][next][parent][TOC]

### TEXTBLTINFO Field - pGlyphIndicies

pGlyphIndicies (PLONG) Pointer to glyph indices.

This string can also be modified based on lGlyphCnt conditions. Refer to GLYPHINFO for example structures to access glyph information. The lowest byte is used to access the low byte table and the 2nd to lowest byte is used to access the high byte table.