## Physical Device Driver Reference

[prev][next][parent][TOC]

### RMGetSnoopLevel

Select an item:

    Calling Sequence
    Calling Parameters
    Returns
    Remarks
    Glossary

This rminfo service gets the next boot and default snoop level for the system. RMSaveDetectedData must save the previous.dat file before the snoop levels can be returned.

    #include <os2.h>

    #include <rmcalls.h>

    USHORT    SnoopLevel;

    USHORT    SnoopFlags;

    APIRET    rc;

    rc = RMGetSnoopLevel(SnoopLevel, SnoopFlags);