## Graphics Adapter Device Driver Reference

[prev][next][parent][TOC]

### MONITORMODEINFO

Contains information on the types of monitor modes.

    typedef struct _MONITORMODEINFO {

      USHORT     usXResolution;  /*  Horizontal pixels. */

      USHORT     usYResolution;  /*  Vertical scan lines. */

      BYTE       bVertRefresh;   /*  Vertical refresh rate. */

      BYTE       bHorizRefresh;  /*  Horizontal refresh rate. */

      BYTE       bVPolarityPos;  /*  Vertical polarity. */

      BYTE       bHPolarityPos;  /*  Horizontal polarity. */

      USHORT     usScrnTop;      /*  Vertical blanking away from the top, in line counts. */

      USHORT     usScrnBottom;   /*  Vertical blanking away from the bottom, in line counts. */

      USHORT     usScrnLeft;     /*  Horizontal blanking away from the left, in pixel counts. */

      USHORT     usScrnRight;    /*  Horizontal blanking away from the right, in pixel counts. */

    } MONITORMODEINFO;

    typedef   MONITORMODEINFO   * FAR   * PMONITORMODEINFO ;