## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Read_Disable

This request is issued by MOUSE$ when it no longer accepts Process_Packet or Process_Absolute requests. References to the common-event buffer should be discontinued. However, MOUSE$ can enable the interface again by sending another Read_Enable request. Normally this request is not issued.

Input: AX = Read_Disable function code, 0003H

Output: No specific output for the request.