## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Test-Case Execution

There are two different ways to run APM tests. One way is to run the program from a command file. To run the command file, first make sure you are in the directory in which the files were installed and then type TEST. The command file will run all of the script files. However, if you would like to test certain parts of the driver, then you need to execute the corresponding test script. For instance, in order to test the function 61 you need to type, 61.CMD.

Another way to run APM IOCtl tests is to run each script file individually. To run one script file at a time, see Description of Test Cases for a description of each script file. After deciding on a script file to run, type in DDTT followed by the script file name:

       [C:\tstapm]DDTT ENABLE01.SCR

After the script has finished executing, control will transfer back to the OS/2 window.