## Physical Device Driver Reference

[prev][next][parent][TOC]

### RMModifyNodeFlags - Calling Parameters

hDriver (HDRIVER) - input Driver handle of the enumerator/snooper driver that creates this adapter.

hNode (RMHANDLE) - input The handle to the resource manager node that needs to be modified. The following types of nodes are valid: Adapter, Device, Detected, Logical Device, System Device.

Flags (USHORT) - input The modified flag value for a given node.

rc (APIRET) - returns On systems where the Resource Manager driver is not installed, the library interface code will return RMRC_NOT_INSTALLED.

RMRC_BAD_DRIVERHANDLE
RMRC_BAD_RMHANDLE
RMRC_SUCCESS