## Physical Device Driver Reference

[prev][next][parent][TOC]

### 11h - Remarks

On entry, the unit code identifies the drive number to be reset. The physical device driver must perform the following actions:

Set the status WORD in the request header
Reset the error condition for the drive

Before this command, the physical device driver had returned the error Uncertain Media for the drive. This action informs the driver that it no longer needs to return the error for the drive.