## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreResetDC Parameter - flOptions

flOptions (ULONG) - input Option flags.

Valid flags are:

RDC_SETOWNERTOSHELL When set, the graphics engine sets the ownership of the reset DC to the process that first initialized the engine, (normally the Presentation Manager interface).

RDC_RGBMODE Sets the DC's logical color table to RGB mode.