## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplProtXlateCmd Parameter - pOutData

pOutData (PVOID) - output Return buffer.

If PD_ALERT is set, this returns a PRTALERT structure. See BIDI_WAIT_ALERT( 8016h) in BIDI Command Structures and Command Flow for more information and Data Types for details on this data structure.

If PD_ALERT is not set, nothing is returned in this buffer.