## Physical Device Driver Reference

[prev][next][parent][TOC]

### CDROMDISK_DEVICESTATUS (60h) - Device Status

Category:
IOCTL_CDROMDISK (80h)
Function:
CDROMDISK_DEVICESTATUS (60h)
Description:
Device Status

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format
    Returns
    Remarks

This function returns the drive-and-door-open status as a doubleword set of bits in the data buffer. This function is performed regardless of whether the drive is already playing.