## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Set Font - Function 10Bh

Category:
Function:
10Bh
Description:
Set Font

Select an item:

    Description
    Parameter Packet Format
    Returns
    Remarks

This function sends a user font definition to the device handler. If the font is appropriate for the current mode, it is loaded into the adapter. If not, it is saved for possible use on subsequent calls to SetMode. The format of the font definition is determined by the type of adapter.