## Physical Device Driver Reference

[prev][next][parent][TOC]

### DSK_DISKETTECONTROL (5Dh) - Remarks

If pending requests are detected, then the handling is up to the tape application. It is recommended that the tape application do an orderly clean-up of its activities and then issue a RESUME IOCTL to allow diskette requests to proceed and subsequently issue another SUSPEND IOCTL to reclaim the diskette hardware.