## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Function 101h - Flags

Flags

Defined as follows:

    Bit 0 indicates whether the physical hardware is

          updated.

          OFF = Initialize only the environment buffer.

          ON  = Initialize the environment buffer and the

                hardware state.

    Bit 1 indicates whether the 3xBox is being

          initialized.

          OFF = The 3xBox is not being initialized.

          ON  = The 3xBox is being initialized.

    Bits 2 thru 15 are reserved and must be OFF.