## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### VDHPopInt

Select an item:

    Format
    Parameters
    Return Codes
    Purpose
    Glossary

This function reverses the effects of VDHPushInt. It removes the Interrupt Return (IRET) frame from the client's stack and restores the client's CS:IP to what was in the IRET frame.

    #include mvdm.h

    VOID    ;

    BOOL    rc;

    rc = VDHPopInt();