## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRTSTARTJOB

Information regarding the job about to be sent to the printer. This information is passed to the BIDI_STARTJOB command.

    typedef struct _PRTSTARTJOB {

      ULONG     ulSpoolerJobID;   /*  Spooler job identifier. */

      ULONG     ulInterpreterID;  /*  Interpreter identifier. */

      ULONG     ulStartPage;      /*  Page in job to begin printing. */

      ULONG     ulEndPage;        /*  Page in job to stop printing. */

    } PRTSTARTJOB;

    typedef   PRTSTARTJOB   * PPRTSTARTJOB ;