## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### ALP3301: Label must be followed by a directive

A user identifier appeared in the label field, but the end of line was encountered before an assembler directive was specified to give the label a definition.

Recovery: Code labels must be followed by a single colon (:) or double colon (::) on the same line as the label itself. Named assembler directives must appear on the same line as the associated label, or the line continuation (\) character must follow the label to create a single logical line.

Check for a possible misspelled identifier or keyword. Verify that the identifier was specified using the correct uppercase and lowercase letters if case sensitive assembly is in effect.