lpadmin(8)

NAME
lpadmin - configure cups printers and classes

SYNOPSIS
lpadmin [ -E ] [ -U username ] [ -h server[:port] ] -d destination
lpadmin [ -E ] [ -U username ] [ -h server[:port] ] -p destination [ -R name-default ] option(s)
lpadmin [ -E ] [ -U username ] [ -h server[:port] ] -x destination

DESCRIPTION
lpadmin configures printer and class queues provided by CUPS. It can also be used to set the server default printer or class.

When specified before the -d, -p, or -x options, the -E option forces encryption when connecting to the server.

The first form of the command (-d) sets the default printer or class to destination. Subsequent print jobs submitted via the lp(1) or lpr(1) commands will use this destination unless the user specifies otherwise with the lpoptions(1) command.

The second form of the command (-p) configures the named printer or class. The additional options are described below.

The third form of the command (-x) deletes the printer or class destination. Any jobs that are pending for the destination will be removed and any job that is currently printed will be aborted.

OPTIONS
The following options are recognized when configuring a printer queue:

-c class
    Adds the named printer to class. If class does not exist it is created automatically.

-i interface
    Sets a System V style interface script for the printer. This option cannot be specified with the -P option (PPD file) and is intended for providing support for legacy printer drivers.

-m model
    Sets a standard System V interface script or PPD file for the printer from the model directory or using one of the driver interfaces. Use the -m option with the lpinfo(8) command to get a list of supported models. The model "raw" clears any existing interface script or PPD file and the model "everywhere" queries the printer referred to by the specified IPP device-uri.

-o cupsIPPSupplies=true

-o cupsIPPSupplies=false
    Specifies whether IPP supply level values should be reported.

-o cupsSNMPSupplies=true

-o cupsSNMPSupplies=false
    Specifies whether SNMP supply level (RFC 3805) values should be reported.

-o job-k-limit=value
    Sets the kilobyte limit for per-user quotas. The value is an integer number of kilobytes; one kilobyte is 1024 bytes.

-o job-page-limit=value
    Sets the page limit for per-user quotas. The value is the integer number of pages that can be printed; double-sided pages are counted as two pages.

-o job-quota-period=value
    Sets the accounting period for per-user quotas. The value is an integer number of seconds; 86,400 seconds are in one day.

-o job-sheets-default=banner

-o job-sheets-default=banner,banner
    Sets the default banner page(s) to use for print jobs.

-o name=value
    Sets a PPD option for the printer. PPD options can be listed using the -l option with the lpoptions(1) command.

-o name-default=value
    Sets a default server-side option for the destination. Any print-time option can be defaulted, e.g., "-o number-up-default=2" to set the default "number-up" option value to 2.

-o port-monitor=name
    Sets the binary communications program to use when printing, "none", "bcp", or "tbcp". The default program is "none". The specified port monitor must be listed in the printer's PPD file.

-o printer-error-policy=name
    Sets the error policy to be used when the printer backend is unable to send the job to the printer. The name must be one of "abort-job", "retry-job", "retry-current-job", or "stop-printer". The default error policy is "stop-printer" for printers and "retry-current-job" for classes.

-o printer-is-shared=true

-o printer-is-shared=false
    Sets the destination to shared/published or unshared/unpublished. Shared/published destinations are publicly announced by the server on the LAN based on the browsing configuration in cupsd.conf, while unshared/unpublished destinations are not announced. The default value is "true".

-o printer-op-policy=name
    Sets the IPP operation policy associated with the destination. The name must be defined in the cupsd.conf in a Policy section. The default operation policy is "default".

-R name-default
    Deletes the named option from printer.

-r class
    Removes the named printer from class. If the resulting class becomes empty it is removed.

-u allow:{user|@group}{,user|,@group}*

-u deny:{user|@group}{,user|,@group}*

-u allow:all

-u deny:none
    Sets user-level access control on a destination. Names starting with "@" are interpreted as UNIX groups. The latter two forms turn user-level access control off.

-v "device-uri"
    Sets the device-uri attribute of the printer queue. Use the -v option with the lpinfo(8) command to get a list of supported device URIs and schemes.

-D "info"
    Provides a textual description of the destination.

-E  Enables the destination and accepts jobs; this is the same as running the cupsaccept(8) and cupsenable(8) programs on the destination.

-L "location"
    Provides a textual location of the destination.

-P ppd-file
    Specifies a PostScript Printer Description file to use with the printer. If specified, this option overrides the -i option (interface script).

CONFORMING TO
Unlike the System V printing system, CUPS allows printer names to contain any printable character except SPACE, TAB, "/", or "#". Also, printer and class names are not case-sensitive. Finally, the CUPS version of lpadmin may ask the user for an access password depending on the printing system configuration. This differs from the System V version which requires the root user to execute this command.

NOTES
The CUPS version of lpadmin does not support all of the System V or Solaris printing system configuration options.

EXAMPLE
Create an IPP Everywhere print queue:
    lpadmin -p myprinter -E -v ipp://myprinter.local/ipp/print -m everywhere

SEE ALSO
cupsaccept(8), cupsenable(8), lpinfo(8), lpoptions(1), CUPS Online Help (http://localhost:631/help)

COPYRIGHT
Copyright © 2007-2015 by Apple Inc.